¡ñ|JadoJd t¡ daaq asea|d ‘ao¡nJas a|es

-la je cnpoJd aq jo acuap¡ a ueHodiu¡ aq s¡ \uauJnoop s¡q\





.I°0°H

(lndu! a0e›Io JadoJduJ¡‘duJnq ’uo¡IeJados¡uJ pa)sJo ca uewnq Áq pasnec pa6euJap aqt@

lnnpoJd aIquJasses!p JauJnsuo0@ '|enueuJ all o||oj ,usei jsqj aõ9sn all Jo uieluieiJJ‘uo¡Te/uasaJd

paleudoJddeu¡ JauJoTsno áq pasneo ueopq9aJq Jo a9uJep aqt@

po!Jad auueualu¡euJ aah Jo a¢!wJas aw!tuaIIa puoáaqo

:ao¡nJas 6uo|aq you saop a6ueg



uo¡ tetiJauJa|d uJ¡ ’XJjsripu | uo¡|eiJJJoju| jo /\Jjs¡u¡|nj /'|ju!o! g |kg\/ siseq

;ouoieuawadwipueqtmaoueidmooaqjiAuedwoono Janaq stsaiaTuiinoAloaToid otpue pa‹,ovunpueNa;esTonpoid

I\yue4ae/n \* T!ieng s}onpoJ,j

#### ”u!x \* pue saga ot /iJnfu! asneo XeuJ uo!i !pe lan

‘aiJJ¡t 6uo| u! aJnsodxa pue }v+!I A y aqt te /i|}oaJip qoo| JaAaN

a6euJep uJoJt sTuaTuoduJoc |euJaTu| agt

TcatoJd o\ u0!u ooh s¡ beau uauv Jamod Tnd\no acnpaJ X||ec¡teuJoTne

|| ’U^ !\\*• nj UO|]oaTap teaqJa o |euJaTu¡ ql¡v sauJoo au¡qceuJ all

e uatin duJe| |¡e u aq t asn ot tou asea|¿g

6u| eai uaqv ’Jajdepe aq} 6n|dun asea|g

Msm i,uc›p osoaty'uoituun; io mo uoqmq latug umum

s 90

#### uJusor +s9c gt6ua|

uJuJC0 L ^Z 08^0 LB.az!S yg t//\jr¿gig:tnd}no pates

#### y r Ho9/os oe/\o#z-oo I :T ndu!

(Jotdepe Sq paJavod ) 'y'g y//\jz¿gg :tndui

### NOi‹cna‹sNI SO

•+!I +^!+fl•°ic svoqs t¡ ’ 6uiuJ¡T u°!icnpu! paleJjui pue s66 • qj uaqy auJ¡T uvopjunoc svogs Xe|dsip aqT ‘ flor 6u!+!i \*o9’\*oc’ o f uag/y\ auJ¡t 6u¡puodsaJJoo agt s^^oqs X9 ds¡p ahi

aseaJou¡ X||ec¡teuJojne Jacob tndtno ’apouJ yeah Koi Joy ( ss o)uo\l nq 6u!+!\ 866 SS+\* d I\* fiS a|qnop ot suJn Javod aft 's¿ Joy uonnq 6u¡+ !T ^66 ^^6Jd 6uoq

/\JouJauJ art Jea|c o\ tJoT\nq 6u¡+ !I °•vi° Jo S¿ oot tJ¡ e6e uo\lnq aqT ssaJ¿ s8 Jot uonnq art ssaJd 6Uo| Xq 6u!+ !i 6u¡puodsaJJoc o\u¡ \a6

au¡qce \/j ”u°!ic unj XJouJauJ auJ¡t qt¡v ale uoTtnq 6u¡uJ!i so9 \*oc \*o r

'SOA t SI 6LtJ|]

6uiqJov xepj”uottnq 6ui+!i 6u!•• aJd tnom!^^ au!v\*• uJ any otui la6 spueq uagm duJe| aft stJe\s X||ec¡\euJolne Josuas paJeJ|u |

jasaJ laulu ||e ’uoT\nq 6uiuJ¡\ amy 0u!ssaJd /iq a\e\s Xqpuets oT sJatua i! ‘ •+!T P^›tas qceaJ ot s|¡ej au¡gceuJ agt

(apow

o| si uo\\nq s66) S66’so ’soc’so r ! Uottnq ^•!+!i •°++°og

sfiets au¡qo9uJ any Jajj9 uoilnq a !i 6u!xJ ov tas ueo slashg

0

JaTdep§ g g tcauuog

### NOizcnazsNl

SO

” |a 6 g gn/ • pi!ng/|a6 /\g aJ nc tcajJ ad p|n og 'salad xa ||9u |euo! satoJd Joy p au ! ag

NOi‹onu‹sNi

Javod a|qnog aporu yeah not/6ui •!t \*66

uo nq 6uitug uo nq 6uitug uo nq 6uitug sq

uogonp°! P° e ;u

oi‹cnuzs i

suo!i on J} su|

,odepg Apoq

0



¡salty og |nyru>^H-UON

## 1VRNVW S‹O3SU



oaten **:NOl1dO 1SblJ bFlOA**


# 0



MAGIC

UV

YOUR FIRST OPTION: UVLED



USER’S MANUAL

Non-Harmful To Eyes!

##### PACKING LIST

Main body DC Adaptor Instru ctions

PARTS INSTRUCTION

Infrared induction

02

Power indicator light 1 0s timinp button 30s timinp button G0s timing button

99s timi ng/Low heat mode Double power

Adapter connection


##### PRODUCT INSTRUCTION

Desig ned for profession al n ail exp erts. CouI d perfect c ure UV geI/Builder/LED gel.

03

04

##### OPERATION INSTRUCTION

Connect D.C Adapter.

Users can set working time by timing button after the machine starts.

Common timing button is 10S,30S,60S,99s (99s button is low

heat mode).

When the machine fails to reach setted time , it enters to standby

state by pressing the timing button, all timer reset.

Infrared sensor automatically starts the lamp when hands get into the machine without pressing timing button.Max working time is 120S.

10s,30s,60stiming button are with time memory function. Machine get into corresponding timing by long press the button for 2s.

Press the button again for 2S or other timing button to clear the memory.

Long press 99s timing button for 2s, the power turns to double. Short Press 99s timing button(0.5s) for low heat mode, output Power automatically increase .

The display shows the corresponding time .When 10s,30s,60s timing work , the display shows countdown time. When the 99s and infrared induction timing, it shows clockwise time.

0

##### TECHNICAL INSTRUCTION

36 LED s

Maximum power consumption: 48W

Machine input: DC24V/1.5A ( powered by adaptor) Adapter:Rated input: 100-240Vac 50/60H z 1A

Rated outp ut:DC24V/1.5A

Size:210x207x103mm Wave length: 365+405nm

**CAUTIONS**

Please read the instruction carefully Defors usinp the lamp

06

Please use the correctly.

Not allow any liquid into the machine u›therwise,damape

#### may ‹Occur.

When timer buttcnn out of function, Please didn’t use.

Please unplug the adapter, when leaving.

Please not to use the nail lamp wten adapter failur e.

net to turn on the machine excess than G00minutes,

otherwise it may reduce the lifetime of nail lamp.

The machine comes with internal overheat detection function,it automatically reduce output power when heat is too high to protect the internal compontents from damage.

Never look directly at the UV light and exposure in long time. UV radiation may cause injury to eyes and skin.

Products Quality Warranty

thank you for choosing U\/LED, in order to make you use this product safely and unworried, and to protect your interests better, our company will be compliance with and implementation of

basic AQSIQ jointly Ministry of Information Industry, implementation after-sale service

@beyond effective service or free maintenance period

@The damae or breakdown caused by customer inappropriated preservation,maintain or the usage that hasn’t follow the manual.

@Consumer disassemble product

@The damaged caused by human factors(ed.misoperation, bump,improper voltage input)

Model: Date of Purchase:

Dealer: Marne:

TEL:

Address:

C This document is the important evidence of the product after-